5078-S.E AMH KLIP BUR 092

**ESSB 5078** - H AMD **1220**

By Representative Klippert

**WITHDRAWN 03/04/2022**

 On page 7, line 33, after "than" strike "10" and insert "15"

On page 7, line 39, after "than" strike "10" and insert "15"

|  |  |
| --- | --- |
|  |  EFFECT:   Modifies the definition of "large capacity magazine" to mean an ammunition feeding device with the capacity to accept more than 15 rounds of ammunition. Modifies the exception to this definition for permanently altered ammunition feeding devices to cover devices altered so they cannot accommodate more than 15 rounds of ammunition. |

**--- END ---**