1100-S AMH MORR HUGH 070

**SHB 1100** - H AMD **540**

By Representative Morris

 On page 4, line 22, after "systems" strike ". This term covers" and insert ", including"

 On page 4, beginning on line 24, after "them." strike all material through "battery." on line 29

 On page 5, beginning on line 9, after "(29)" strike all material through "(30)" on line 24

 Renumber the remaining subsections consecutively and correct any internal references accordingly.

 On page 5, beginning on line 36, after "less" strike all material through "power" on line 38

 On page 5, beginning on line 38, after "power." strike the remainder of the section

 On page 6, line 31, after "cabinets;" insert "and"

 On page 6, beginning on line 32, after "(j)" strike all material through "(k)" on line 33

 Renumber the remaining subsections consecutively and correct any internal references accordingly.

 On page 6, line 38, after "thereof" strike ". This exception does not apply" and insert ", including"

 On page 7, line 13, after "analyzers;" strike "or"

 On page 7, beginning on line 17, after "section;" strike all material through "filters" on line 20 and insert "or

 (vii) Used to charge larger industrial motive equipment such as fork lifts, burden carriers, or person carriers"

 On page 12, beginning on line 9, after "section." strike the remainder of the section

 On page 14, beginning on line 33, strike all of section 5

 Correct the title.

|  |  |
| --- | --- |
|  |  EFFECT:  Removes all references to and efficiency standards for high light output double-ended quartz halogen lamps, small diameter directional lamps, state-regulated LED lamps, and HVAC air filters. Extends an exception from the efficiency standards established for battery charger systems to those used to charge autoettes or electric personal assistive mobility devices, golf carts, low-speed vehicles, and larger industrial motive equipment such as fork lifts, burden carriers, or person carriers. Removes the requirement for the Department of Commerce to report on standards for high light output double-ended quartz halogen lamps.  |

**--- END ---**