**1841 AMS KING S7572.2 - NOT FOR FLOOR USE**

**HB 1841** - S AMD TO S AMD (S-7432.1/20) **1347**

By Senator King

**ADOPTED 03/06/2020**

On page 1, line 24, after "(2)" insert "Class III" means a railroad carrier designated as a class III railroad by the United States surface transportation board.

(3)"

Renumber the remaining subsections consecutively and correct any internal references accordingly.

On page 2, at the beginning of line 8, insert "(1)"

On page 2, after line 14, insert the following:

"(2) Class III railroad carriers operating on their roads while at a speed of twenty-five miles per hour or less are exempt from subsection (1) of this section."

EFFECT: Exempts Class III railroad carriers operating on their roads while at a speed of twenty-five miles per hour or less from the 2 crewmember requirement.