**1782-S AMH CALD H2691.2 - NOT FOR FLOOR USE**

**SHB 1782** - H AMD TO H AMD (H-2689.4/22) **1038**

By Representative Caldier

On page 13, at the beginning of line 18, strike "of 30,000" and insert "of 700,000"

On page 13, line 20, after "population of" strike "30,000" and insert "700,000"

On page 20, at the beginning of line 11, strike "of 30,000" and insert "of 700,000"

On page 20, line 13, after "population of" strike "30,000" and insert "700,000"

EFFECT: Raises the population threshold for middle housing requirements and certain housing element requirements to 700,000.