S-4060.1

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**SUBSTITUTE SENATE BILL 6284**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**State of Washington 64th Legislature 2016 Regular Session**

**By** Senate Government Operations & Security (originally sponsored by Senators Takko and Roach)

AN ACT Relating to preventing water-sewer districts from prohibiting multipurpose fire sprinkler systems; and adding a new section to chapter 57.02 RCW.

BE IT ENACTED BY THE LEGISLATURE OF THE STATE OF WASHINGTON:

NEW SECTION. **Sec.**  A new section is added to chapter 57.02 RCW to read as follows:

(1) A water-sewer district may not prohibit the use of multipurpose fire sprinkler systems that are part of a structure's plumbing system for single-family homes and townhouses as defined by the state residential building code or require a separate water meter or backflow preventer for the multipurpose fire sprinkler system.

(2) For the purposes of this section, "multipurpose fire sprinkler system" means a fire sprinkler system that:

(a) Is supplied only by the purveyor's water;

(b) Does not have a fire department pumper connection;

(c) Is constructed of approved potable water piping and materials to which sprinkler heads are attached; and

(d) Terminates at a connection to a toilet or other plumbing fixture to prevent stagnant water.

**--- END ---**